Model 348 Dante Firmware

File Name: M348v2r4r0.dnt

Version History:

Version: 2.4.0
Release Date: 09-Jun-2026
Description: Disables Telnet FTP access. Maintenance release which provides important bug fixes for devices that are enrolled in managed Dante networks. (Broadway Firmware v4.2.9.1)

Version: 2.3.0
Release Date: 26-Jul-2022
Description: Adds Tally Tone Dante transmitter (output) channel. Rquires use of Main Firmware v2.05 and later. (Broadway Firmware v4.2.6.4)

Version: 2.2.2
Release Date: 04-May-2021
Description: Renames Dante receiver (input) channel "IFB Pgm 8" to "Aux In". (When Model 348 uses Main Firmware version 2.00, the Aux In channel can be used as either a Microphone or IFB source). Includes a recommended maintenance release of the Broadway firmware which provides a range of bug fixes. (Broadway Firmware v4.2.6.4)

Version: 2.1.0
Release Date: 05-May-2020
Description: Maintenance release which provides a range of bug fixes. (Broadway Firmware v4.2.4.2)

Version: 2.0.0
Release Date: 16-Sep-2019
Description: Adds support for SMPTE ST 2110-30 RTP audio transport for DDM-enrolled devices. Adds support for AES67 RTP audio transport for DDM-enrolled devices. Adds dynamic enable/disable of AES67 mode. Adds support for "wide flows"; Tx multicast flows can now be created with up to 16 channels. Adds support for redundant RTP multicast flows. Includes many bug fixes and general improvements. (Broadway Firmware v4.2.1.8)

Version: 1.1.0
Release Date: 01-Aug-2019
Description: Adds eight IFB Program input (Dante receiver (input)) channels. Adds Hot Mic output (Dante transmitter (output)) channel. Renames Monitor Output 1 and 2 to Monitor Output A and B. Requires Model 348 Main Firmware v1.04 and later. Supported using STcontroller v2.03.00 and later. (Broadway v4.0.9.2)

Version: 1.0.0
Release Date: 17-May-2019
Description: Initial Release. (Broadway v4.0.9.2)
