Model 5422A-02 Dante Firmware

File Name: M5422A-02v3r0r0.dnt

Version History:

Version: 3.0.0
Release Date: 09-Feb-2026
Description: Adds support for SMPTE ST 2110-30 in unmanaged mode and PTPv2 manual clocking configuration. Changes default switch configuration to Redundant. Updates custom link status application to support new Brooklyn 3 firmware. (Brooklyn 3 Firmware v4.3.1.8)

Version: 2.1.0
Release Date: 07-Aug-2024
Description: Various back-end improvements and bug fixes. (Brooklyn 3 Firmware v4.2.8.9)

Version: 2.0.0
Release Date: 08-Dec-2023
Description: Initial Release for Brooklyn 3. Disables Telnet Access. (Brooklyn 3 Firmware v4.2.7.7)

